{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Control"],"not_rendered":{"charts":2,"images":1,"macros":1,"external_links":0,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Control","index":0,"n_rows":89,"n_cols":4,"rows_kept":89,"cut":false,"hidden":false,"merged":[[10,1,10,3],[11,1,11,3],[12,1,12,3],[13,0,13,3],[5,0,5,3],[6,1,6,3],[7,1,7,3],[8,1,8,3],[9,0,9,3],[3,9,3,11],[4,1,4,3],[2,1,2,3],[3,1,3,3],[0,1,0,3],[1,0,1,3]]}
["Status:","Failed to find HAMEG Instruments, HM8118, is it connected?"]
["LCR bridge"]
["COM Port:",1]
["Baudrate:",9600]
["Device","<No response from instrument!>"]
["Power supply"]
["COM Port:",1]
["Baudrate:",9600]
["Device","<No response from instrument!>"]
["Bench meter"]
["COM Port:",1]
["Baudrate:",9600]
["Device","<No response from instrument!>"]
["Test Settings"]
["Delay:",100,"milliseconds"]
["Run Length:",69]
[]
[]
[]
["Frequency","Result 1:","Result 2:","Result 3:"]
[20]
[24]
[25]
[30]
[36]
[40]
[45]
[50]
[60]
[72]
[75]
[80]
[90]
[100]
[120]
[150]
[180]
[200]
[240]
[250]
[300]
[360]
[400]
[450]
[500]
[600]
[720]
[750]
[800]
[900]
[1000]
[1200]
[1500]
[1800]
[2000]
[2400]
[2500]
[3000]
[3600]
[4000]
[4500]
[5000]
[6000]
[7200]
[7500]
[8000]
[9000]
[10000]
[12000]
[15000]
[18000]
[20000]
[24000]
[25000]
[30000]
[36000]
[40000]
[45000]
[50000]
[60000]
[72000]
[75000]
[80000]
[90000]
[100000]
[120000]
[150000]
[180000]
[200000]